{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":69,"n_cols":29,"rows_kept":69,"cut":false,"hidden":false,"merged":[[28,20,28,21],[28,25,28,26],[2,0,3,4],[5,15,5,16],[28,0,28,1],[28,5,28,6],[28,10,28,11],[28,15,28,16],[43,10,43,11],[5,0,5,1],[5,5,5,6],[5,10,5,11]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
["RADIO A",{"$nulls":4},"RADIO B",{"$nulls":4},"RADIO C",{"$nulls":4},"RADIO D"]
["D-SUB15",{"$nulls":4},"D-SUB15",{"$nulls":4},"D-SUB15",{"$nulls":4},"D-SUB15"]
[1,"BAND DATA 1","BCD1A","IN",null,1,"BAND DATA 1","BCD1B","IN",null,1,"BAND DATA 1","BCD1C","IN",null,1,"BAND DATA 1","BCD1D","IN"]
[2,"BAND DATA 2","BCD2A","IN",null,2,"BAND DATA 2","BCD2B","IN",null,2,"BAND DATA 2","BCD2C","IN",null,2,"BAND DATA 2","BCD2D","IN"]
[3,"BAND DATA 3","BCD3A","IN",null,3,"BAND DATA 3","BCD3B","IN",null,3,"BAND DATA 3","BCD3C","IN",null,3,"BAND DATA 3","BCD3D","IN"]
[4,"BAND DATA 4","BCD4A","IN",null,4,"BAND DATA 4","BCD4B","IN",null,4,"BAND DATA 4","BCD4C","IN",null,4,"BAND DATA 4","BCD4D","IN"]
[5,"PAPTT","PAPTTA","IN",null,5,"PAPTT","PAPTTB","IN",null,5,"PAPTT","PAPTTC","IN",null,5,"PAPTT","PAPTTD","IN"]
[6,"ALARM","ALMA","OUT",null,6,"ALARM","ALMB","OUT",null,6,"ALARM","ALMC","OUT",null,6,"ALARM","ALMD","OUT"]
[7,"POWER","PWRA","AN OUT",null,7,"POWER","PWRB","AN",null,7,"POWER","PWRC","AN",null,7,"POWER","PWRD","AN"]
[8,"RESET","RESETA","OUT",null,8,"RESET","RESETB","OUT",null,8,"RESET","RESETC","OUT",null,8,"RESET","RESETD","OUT"]
[9,"RADIO PTT","RAPTTA","IN",null,9,"RADIO PTT","RAPTTB","IN",null,9,"RADIO PTT","RAPTTC","IN",null,9,"RADIO PTT","RAPTTD","IN"]
[10,"SPARE IO 1","AUXA1",null,null,10,"SPARE IO 1","AUXB1",null,null,10,"SPARE IO 1","AUXC1",null,null,10,"SPARE IO 1","AUXD1"]
[11,"SPARE IO 2","AUXA2",null,null,11,"SPARE IO 2","AUXB2",null,null,11,"SPARE IO 2","AUXC2",null,null,11,"SPARE IO 2","AUXD2"]
[12,{"$nulls":4},12,{"$nulls":4},12,{"$nulls":4},12]
[13,{"$nulls":4},13,{"$nulls":4},13,{"$nulls":4},13]
[14,{"$nulls":4},14,{"$nulls":4},14,{"$nulls":4},14]
[15,{"$nulls":4},15,{"$nulls":4},15,{"$nulls":4},15]
[]
[]
[]
[]
[]
[]
["PA 10M",{"$nulls":4},"PA 15M",{"$nulls":4},"PA 20M",{"$nulls":4},"PA 40M",{"$nulls":4},"PA 80M",{"$nulls":4},"PA 160M"]
["D-SUB9",{"$nulls":4},"D-SUB9",{"$nulls":4},"D-SUB9",{"$nulls":4},"D-SUB9",{"$nulls":4},"D-SUB9",{"$nulls":4},"D-SUB9"]
[1,"PA PTT 10M ","PAPTT10","OUT",null,1,"PA PTT 15M ","PAPTT15","OUT",null,1,"PA PTT 20M ","PAPTT20","OUT",null,1,"PA PTT 40M ","PAPTT40","OUT",null,1,"PA PTT 80M ","PAPTT80","OUT",null,1,"PA PTT 160M ","PAPTT160","OUT"]
[2,"PA POWER 10M","PWR10","AN IN",null,2,"PA POWER 15M","PWR15","AN IN",null,2,"PA POWER 20M","PWR20","AN IN",null,2,"PA POWER 40M","PWR40","AN IN",null,2,"PA POWER 80M","PWR80","AN IN",null,2,"PA POWER 160M","PWR160","AN IN"]
[3,"PA RESET 10M","RESET10","OUT",null,3,"PA RESET 15M","RESET15","OUT",null,3,"PA RESET 20M","RESET20","OUT",null,3,"PA RESET 40M","RESET40","OUT",null,3,"PA RESET 80M","RESET80","OUT",null,3,"PA RESET 160M","RESET160","OUT"]
[4,"PA ALARM 10M","ALM10","IN",null,4,"PA ALARM 15M","ALM15","IN",null,4,"PA ALARM 20M","ALM20","IN",null,4,"PA ALARM 40M","ALM40","IN",null,4,"PA ALARM 80M","ALM80","IN",null,4,"PA ALARM 160M","ALM160","IN"]
[5,"SPARE IO 1","AUX1010",null,null,5,{"$nulls":4},5,{"$nulls":4},5,{"$nulls":4},5,{"$nulls":4},5]
[6,{"$nulls":4},6,{"$nulls":4},6,{"$nulls":4},6,{"$nulls":4},6,{"$nulls":4},6]
[7,{"$nulls":4},7,{"$nulls":4},7,{"$nulls":4},7,{"$nulls":4},7,{"$nulls":4},7]
[8,{"$nulls":4},8,{"$nulls":4},8,{"$nulls":4},8,{"$nulls":4},8,{"$nulls":4},8]
[9,{"$nulls":4},9,{"$nulls":4},9,{"$nulls":4},9,{"$nulls":4},9,{"$nulls":4},9]
[]
[]
[]
[]
["ANTENNA RELAYS 4-1",{"$nulls":4},"RADIO RELAY 1-6",{"$nulls":4},"POWER MONITOR",{"$nulls":4},"DISPLAY"]
["D-SUB25",{"$nulls":4},"D-SUB25",{"$nulls":5},"POWER SELECT 1","PWRMTR1","IN",null,1,"LCD CONTROL"]
[1,"RELAY 10M A","RLY10A","OUT",null,1,"RELAY RADIOA 10M","RLYRA10","OUT",null,null,"POWER SELECT 2","PWRMTR2","IN",null,2,"LCD CONTROL"]
[2,"RELAY 10M B","RLY10B","OUT",null,2,"RELAY RADIOA 15M","RLYRA15","OUT",null,null,"POWER SELECT 3","PWRMTR3","IN",null,3,"LCD CONTROL"]
[3,"RELAY 10M C","RLY10C","OUT",null,3,"RELAY RADIOA 20M","RLYRA20","OUT",null,null,"POWER METER OUT","PWROUT","AN OUT",null,4,"LCD CONTROL"]
[4,"RELAY 10M D","RLY10D","OUT",null,4,"RELAY RADIOA 40M","RLYRA40","OUT",null,null,"RADIO TUNE PTT","TUNE","IN",null,5,"LCD CONTROL"]
[5,"RELAY 15M A","RLY15A","OUT",null,5,"RELAY RADIOA 80M","RLYRA80","OUT",{"$nulls":6},6,"LCD CONTROL"]
[6,"RELAY 15M B","RLY15B","OUT",null,6,"RELAY RADIOA 160M","RLYRA160","OUT",{"$nulls":6},7,"LCD CONTROL"]
[7,"RELAY 15M C","RLY15C","OUT",null,7,"RELAY RADIOB 10M","RLYRB10","OUT",{"$nulls":6},8,"LCD CONTROL"]
[8,"RELAY 15M D","RLY15D","OUT",null,8,"RELAY RADIOB 15M","RLYRB15","OUT",{"$nulls":6},9,"BUTTON 1"]
[9,"RELAY 20M A","RLY20A","OUT",null,9,"RELAY RADIOB 20M","RLYRB20","OUT",{"$nulls":6},10,"BUTTON 2"]
[10,"RELAY 20M B","RLY20B","OUT",null,10,"RELAY RADIOB 40M","RLYRB40","OUT",{"$nulls":6},11,"BUTTON 3"]
[11,"RELAY 20M C","RLY20C","OUT",null,11,"RELAY RADIOB 80M","RLYRB80","OUT",{"$nulls":6},12,"BUTTON 4"]
[12,"RELAY 20M D","RLY20D","OUT",null,12,"RELAY RADIOB 160M","RLYRB160","OUT"]
[13,"RELAY 40M A","RLY40A","OUT",null,13,"RELAY RADIOC 10M","RLYRC10","OUT"]
[14,"RELAY 40M B","RLY40B","OUT",null,14,"RELAY RADIOC 15M","RLYRC15","OUT"]
[15,"RELAY 40M C","RLY40C","OUT",null,15,"RELAY RADIOC 20M","RLYRC20","OUT"]
[16,"RELAY 40M D","RLY40D","OUT",null,16,"RELAY RADIOC 40M","RLYRC40","OUT",null,null,null,0]
[17,"RELAY 80M A","RLY80A","OUT",null,17,"RELAY RADIOC 80M","RLYRC80","OUT",null,null,"Number of INPUT",7]
[18,"RELAY 80M B","RLY80B","OUT",null,18,"RELAY RADIOC 160M","RLYRC160","OUT",null,null,"Number of OUTPUT"]
[19,"RELAY 80M C","RLY80C","OUT",null,19,"RELAY RADIOD 10M","RLYRD10","OUT"]
[20,"RELAY 80M D","RLY80D","OUT",null,20,"RELAY RADIOD 15M","RLYRD15","OUT"]
[21,"RELAY 160M A","RLY160A","OUT",null,21,"RELAY RADIOD 20M","RLYRD20","OUT"]
[22,"RELAY 160M B","RLY160B","OUT",null,22,"RELAY RADIOD 40M","RLYRD40","OUT"]
[23,"RELAY 160M C","RLY160C","OUT",null,23,"RELAY RADIOD 80M","RLYRD80","OUT"]
[24,"RELAY 160M D","RLY160D","OUT",null,24,"RELAY RADIOD 160M","RLYRD160","OUT"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}