{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":201,"n_cols":9,"rows_kept":201,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
["RADIO A"]
["D-SUB15"]
[1,"BAND DATA 1","BCD1A",null,null,null,"RADIO",36,36]
[2,"BAND DATA 2","BCD2A",null,null,null,"RELAY",48,24]
[3,"BAND DATA 3","BCD3A",null,null,null,"PA",24,24]
[4,"BAND DATA 4","BCD4A",null,null,null,"MONITOR",5,5]
[5,"PAPTT","PAPTTA",{"$nulls":4},113,89]
[6,"ALARM","ALMA"]
[7,"POWER","PWRA"]
[8,"RESET","RESETA"]
[9,"RADIO PTT","RAPTTA"]
[10]
[11]
[12]
[13]
[14]
[15]
[]
["RADIO B"]
["D-SUB15"]
[1,"BAND DATA 1","BCD1B"]
[2,"BAND DATA 2","BCD2B"]
[3,"BAND DATA 3","BCD3B"]
[4,"BAND DATA 4","BCD4B"]
[5,"PAPTT","PAPTTB"]
[6,"ALARM","ALMB"]
[7,"POWER","PWRB"]
[8,"RESET","RESETB"]
[null,"RADIO PTT","RAPTTB"]
[]
["RADIO C"]
["D-SUB15"]
[1,"BAND DATA 1","BCD1C"]
[2,"BAND DATA 2","BCD2C"]
[3,"BAND DATA 3","BCD3C"]
[4,"BAND DATA 4","BCD4C"]
[5,"PAPTT","PAPTTC"]
[6,"ALARM","ALMC"]
[7,"POWER","PWRC"]
[8,"RESET","RESETC"]
[9,"RADIO PTT","RAPTTC"]
[]
["RADIO D"]
["D-SUB15"]
[1,"BAND DATA 1","BCD1D"]
[2,"BAND DATA 2","BCD2D"]
[3,"BAND DATA 3","BCD3D"]
[4,"BAND DATA 4","BCD4D"]
[5,"PAPTT","PAPTTD"]
[6,"ALARM","ALMD"]
[7,"POWER","PWRD"]
[8,"RESET","RESETD"]
[9,"RADIO PTT","RAPTTD"]
[]
["ANTENNA RELAYS 4-1"]
["D-SUB25"]
[1,"RELAY 10M A","RLY10A"]
[2,"RELAY 10M B","RLY10B"]
[3,"RELAY 10M C","RLY10C"]
[4,"RELAY 10M D","RLY10D"]
[5,"RELAY 15M A","RLY15A"]
[6,"RELAY 15M B","RLY15B"]
[7,"RELAY 15M C","RLY15C"]
[8,"RELAY 15M D","RLY15D"]
[9,"RELAY 20M A","RLY20A"]
[10,"RELAY 20M B","RLY20B"]
[11,"RELAY 20M C","RLY20C"]
[12,"RELAY 20M D","RLY20D"]
[13,"RELAY 40M A","RLY40A"]
[14,"RELAY 40M B","RLY40B"]
[15,"RELAY 40M C","RLY40C"]
[16,"RELAY 40M D","RLY40D"]
[17,"RELAY 80M A","RLY80A"]
[18,"RELAY 80M B","RLY80B"]
[19,"RELAY 80M C","RLY80C"]
[20,"RELAY 80M D","RLY80D"]
[21,"RELAY 160M A","RLY160A"]
[22,"RELAY 160M B","RLY160B"]
[23,"RELAY 160M C","RLY160C"]
[24,"RELAY 160M D","RLY160D"]
[]
["RADIO RELAY 1-6"]
["D-SUB25"]
[1,"RELAY RADIOA 10M","RLYRA10"]
[2,"RELAY RADIOA 15M","RLYRA15"]
[3,"RELAY RADIOA 20M","RLYRA20"]
[4,"RELAY RADIOA 40M","RLYRA40"]
[5,"RELAY RADIOA 80M","RLYRA80"]
[6,"RELAY RADIOA 160M","RLYRA160"]
[7,"RELAY RADIOB 10M","RLYRB10"]
[8,"RELAY RADIOB 15M","RLYRB15"]
[9,"RELAY RADIOB 20M","RLYRB20"]
[10,"RELAY RADIOB 40M","RLYRB40"]
[11,"RELAY RADIOB 80M","RLYRB80"]
[12,"RELAY RADIOB 160M","RLYRB160"]
[13,"RELAY RADIOC 10M","RLYRC10"]
[14,"RELAY RADIOC 15M","RLYRC15"]
[15,"RELAY RADIOC 20M","RLYRC20"]
[16,"RELAY RADIOC 40M","RLYRC40"]
[17,"RELAY RADIOC 80M","RLYRC80"]
[18,"RELAY RADIOC 160M","RLYRC160"]
[19,"RELAY RADIOD 10M","RLYRD10"]
[20,"RELAY RADIOD 15M","RLYRD15"]
[21,"RELAY RADIOD 20M","RLYRD20"]
[22,"RELAY RADIOD 40M","RLYRD40"]
[23,"RELAY RADIOD 80M","RLYRD80"]
[24,"RELAY RADIOD 160M","RLYRD160"]
[]
["PA 10M"]
["D-SUB9"]
[1,"PA PTT 10M ","PAPTT10"]
[2,"PA POWER 10M","PWR10"]
[3,"PA RESET 10M","RESET10"]
[4,"PA ALARM 10M","ALM10"]
[5]
[6]
[7]
[8]
[9]
[]
["D-SUB9"]
[1,"PA PTT 15M ","PAPTT15"]
[2,"PA POWER 15M","PWR15"]
[3,"PA RESET 15M","RESET15"]
[4,"PA ALARM 15M","ALM15"]
[5]
[6]
[7]
[8]
[9]
[]
["D-SUB9"]
[1,"PA PTT 20M ","PAPTT20"]
[2,"PA POWER 20M","PWR20"]
[3,"PA RESET 20M","RESET20"]
[4,"PA ALARM 20M","ALM20"]
[5]
[6]
[7]
[8]
[9]
[]
["D-SUB9"]
[1,"PA PTT 40M ","PAPTT40"]
[2,"PA POWER 40M","PWR40"]
[3,"PA RESET 40M","RESET40"]
[4,"PA ALARM 40M","ALM40"]
[5]
[6]
[7]
[8]
[9]
[]
["D-SUB9"]
[1,"PA PTT 80M ","PAPTT80"]
[2,"PA POWER 80M","PWR80"]
[3,"PA RESET 80M","RESET80"]
[4,"PA ALARM 80M","ALM80"]
[5]
[6]
[7]
[8]
[9]
[]
["D-SUB9"]
[1,"PA PTT 160M ","PAPTT160"]
[2,"PA POWER 160M","PWR160"]
[3,"PA RESET 160M","RESET160"]
[4,"PA ALARM 160M","ALM160"]
[5]
[6]
[7]
[8]
[9]
[]
["MONITOR"]
[null,"POWER METER 1","PWRMTR1"]
[null,"POWER METER 2","PWRMTR2"]
[null,"POWER METER 3","PWRMTR3"]
[null,"POWER METER OUT","PWROUT"]
[null,"RADIO TUNE PTT","TUNE"]
[]
[]
["DISPLAY"]
[1,"LCD CONTROL"]
[2,"LCD CONTROL"]
[3,"LCD CONTROL"]
[4,"LCD CONTROL"]
[5,"LCD CONTROL"]
[6,"LCD CONTROL"]
[7,"LCD CONTROL"]
[8,"LCD CONTROL"]
[9,"BUTTON 1"]
[10,"BUTTON 2"]
[11,"BUTTON 3"]
[12,"BUTTON 4"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}